Filetype: Flipper SubGhz Setting File
Version: 1

# Add Standard frequencies for your region
Add_standard_frequencies: false

# Default Frequency: used as default for "Read" and "Read Raw"
Default_frequency: 433920000

# Frequencies used for "Read", "Read Raw" and "Frequency Analyzer"
Frequency: 300000000
Frequency: 302757000
Frequency: 303875000
Frequency: 304250000
Frequency: 307000000
Frequency: 307500000
Frequency: 307800000
Frequency: 309000000
Frequency: 310000000
Frequency: 312000000
Frequency: 313000000
Frequency: 313850000
Frequency: 314000000
Frequency: 314350000
Frequency: 315000000
Frequency: 318000000
Frequency: 345000000
Frequency: 348000000
Frequency: 387000000
Frequency: 390000000
Frequency: 418000000
Frequency: 433075000
Frequency: 433220000
Frequency: 433420000
Frequency: 433657070
Frequency: 433889000
Frequency: 433920000
Frequency: 434176948
Frequency: 434420000
Frequency: 434775000
Frequency: 438900000
Frequency: 464000000
Frequency: 779000000
Frequency: 868350000
Frequency: 868400000
Frequency: 906400000
Frequency: 915000000
Frequency: 925000000
Frequency: 928000000

# Frequencies used for hopping mode (keep this list small or flipper will miss signal)
Hopper_frequency: 310000000
Hopper_frequency: 313000000
Hopper_frequency: 315000000
Hopper_frequency: 318000000
Hopper_frequency: 390000000
Hopper_frequency: 433920000
Hopper_frequency: 434420000
Hopper_frequency: 868350000

# Custom preset
# format for CC1101 "Custom_preset_data:" XX YY XX YY .. 00 00 ZZ ZZ ZZ ZZ ZZ ZZ ZZ ZZ, where: XX-register, YY - register data, 00 00 - end load register, ZZ - 8 byte Pa table register
#Custom_preset_name: AM_1
#Custom_preset_module: CC1101
#Custom_preset_data: 02 0D 03 07 08 32 0B 06 14 00 13 00 12 30 11 32 10 17 18 18 19 18 1D 91 1C 00 1B 07 20 FB 22 11 21 B6 00 00 00 C0 00 00 00 00 00 00
#Custom_preset_name: AM_2
#Custom_preset_module: CC1101
#Custom_preset_data: 02 0D 03 07 08 32 0B 06 14 00 13 00 12 30 11 32 10 17 18 18 19 18 1D 91 1C 00 1B 07 20 FB 22 11 21 B6 00 00 00 C0 00 00 00 00 00 00

Custom_preset_name: Honda1
Custom_preset_module: CC1101
#                                                          G2    G3    G4    D                 L0    L1    L2
Custom_preset_data: 02 0D 0B 06 08 32 07 04 14 00 13 02 12 04 11 36 10 69 15 32 18 18 19 16 1D 91 1C 00 1B 07 20 FB 22 10 21 56 00 00 C0 00 00 00 00 00 00 00

Custom_preset_name: Honda2
Custom_preset_module: CC1101
#                                                          G2    G3    G4    D                 L0    L1    L2
Custom_preset_data: 02 0D 0B 06 08 32 07 04 14 00 13 02 12 07 11 36 10 E9 15 32 18 18 19 16 1D 92 1C 40 1B 03 20 FB 22 10 21 56 00 00 C0 00 00 00 00 00 00 00
